Potentiometer: PE5

Dip Switch: PA4

Green LED: PB3

Red LED: PD1 (M1PWM1) --- changed to PB6 (M0PWM0)

PB7 (M0PWM1)